Software Requirements Specification (SRS)

**Automated Pedestrian Collision Avoidance System (APCA)**

Authors: Team GReEN; Garret Smith, Rebecca Collins, Eric Austin, Nikhil Andrews

Customer: Mr. David Agnew, Continental Automotive Systems

**Instructor:** Dr. Betty Cheng, Michigan State University

1. Introduction

This software requirements specification (SRS) document provides an overview of the documents purpose, scope, definitions, acronyms and abbreviations, and the overall organization of this document.

Section 2 gives the overall description of the APCA System. This section includes the product perspective, product function, user characteristics, constraints, assumptions and dependencies, and apportioning of requirements.

The following sections provide the requirements and models of our system (Sections 3 and 4).A demonstration using a prototype; how to run the prototype and sample scenarios are also included (Section 5). Finally, references for this document are identified in Section 6.

* 1. Purpose

The purpose of the SRS is to describe the specifics of the Automated Pedestrian Collision Avoidance system (APCA); how the system behaves, system goals, specification and constraints under which the system operates. This document is mainly intended for those developers working on such systems, but in our case more specifically intended for Mr. David Agnew of Continental Automotive Systems.

* 1. Scope

The Automated Pedestrian Collision Avoidance System (APCA) is an autonomous system that is designed to avoid collisions with pedestrians. This system provides an automated control over the vehicle’s braking system (BBW or Brake-By-Wire) that responds to potential collisions while minimizing loss of efficiency (time). The system also has control over the vehicle’s acceleration in order to return to original speed after avoiding collision. To sum up, APCA is designed to provide additional safety to the driver and pedestrians.

* 1. Definitions, acronyms, and abbreviations

This section of the SRS contains definitions, acronyms, and abbreviations for the terminology used to describe our system throughout this document.

* **APCA** – Automated Pedestrian Collision Avoidance
* **State** – The state the system is in.
* **Pedestrian Sensor** – A stereo camera that provides pedestrian recognition, relative location, speed, and relative direction with respect to the vehicle.
* **Packet** – A piece of data generated by the pedestrian sensor containing the relative locations, speeds, and relative directions of pedestrians in and near the path of the vehicle.
* **Cycle Time** – the time it takes for the pedestrian sensor to send the packet of signals. In the project overview, it is given as 100 ms.
* **Brake-by-Wire** – a sub-system that responds to deceleration requests by interrupting the steady speed (set by cruise control) and then applying brakes.
* **Vehicle** – the autonomous vehicle for this application
* **“Lost time”** – time difference (in seconds) between system on (vehicle starts to avoid collision) and system off (vehicle avoids and returns back to steady state speed).
* **Fail Safe** – or fail operational mode, increases the response time to apply brakes in order to reach the requested deceleration. In the project overview, it is given that response time for braking increases from 200 ms to 900 ms.
  1. Organization

The remainder of this document is organized as follows.

The second section of this document, Overall Description, gives a general idea of how the product functions. Some of the key concepts described are: interface constraints, the intended users, and assumptions.

The third section of this document, Specific Requirements, gives an enumerated list of requirements that the system fulfills.

The fourth section of this document, Modeling Requirements, explains how the software is designed to meet the requirements. In this section, diagrams (Use case, Class, and State) are used to specify how the software functions.

The fifth section, Prototype, provides a demonstration on how to use and run the prototype and includes sample scenarios of the system.

The sixth section, References, gives a list of all documents referenced.

The Last section of this document, Point of Contact, gives information on how to obtain more information regarding this document and project.

1. Overall Description

Autonomous driving is an area of great interest to the auto industry. An essential task of an automated car is to avoid collisions. This is currently performed by human drivers, who respond to hazardous situations. However, an autonomous vehicle cannot rely on human intervention when threats arise. The APCA system uses a stereo camera to detect pedestrians and applies braking automatically if necessary to avoid a collision with the pedestrian.

* 1. Product Perspective

The APCA system is an autonomous safety system used for avoiding collisions with pedestrians. The system detects pedestrians with a stereo camera and tracks their location and path. If a collision is imminent, a signal is sent to the BBW actuator to being braking. The system interfaces with the BWW actuator and with the stereo camera used for pedestrian detection. Since the vehicle is autonomous, no user interface exists for this system. The system is active whenever the vehicle is on, and receives a signal from the stereo camera every 100ms.

* 1. Product Functions

The following are functions of our product as specified by the customer.

Detection: The use of the pedestrian stereo camera to locate pedestrians in front of the vehicle.

Tracking: Using the camera and algorithms, track the position of the pedestrian as it moves within the sensors scanning range.

Apply Braking: When a pedestrian steps in front of the vehicle and a collision is possible, a signal is sent to the BBW actuator to begin deceleration.

Restore Velocity: When the pedestrian threat is gone and braking has been applied, tell the vehicle to restore its previous velocity.

Fail Safe: If there is a problem with braking, the fail safe mode is applied. This increases the time allowed for braking to ensure collisions are avoided.

* 1. User Characteristics

The user in the context of this product would be considered the driver of the vehicle. However, the vehicles that will be equipped with the APCA system will be autonomous. Therefore, the driver is assumed to have little or no knowledge of the system. The driver is also expected to have no interaction with the system.

* 1. Constraints

The APCA system must have zero collisions for each scenario presented as stated in the Project Description. The system must also attempt to avoid time loss due to pedestrian avoidance. This must not interfere with safety constraints however. If a braking problem is present, the APCA system must enable the fail safe system and increase time allowed for braking. Additionally, the BBW actuator is configured to respond to commands as quickly as a human. The response time to reach the requested deceleration is 200ms and the brake release time is 100ms. Also, with the given scenarios, the vehicle will always be travelling at a steady velocity of 13.9 m/s and have an acceleration of .25g after braking is applied.

* 1. Assumptions and Dependencies

Some assumptions were clarified by the customer about the system and elements that interact with it. It is assumed that the APCA system is always on and scanning if the vehicle is running. It is also assumed that the pedestrian will only move at either 0 or 6 kilometer per hour, and their acceleration is infinite. Also, the pedestrian will always be moving at a 90 degree angle to the vehicles path. It is also assumed that the elements of the system are all functioning properly and no abnormal conditions are present.


* 1. Approportioning of Requirements

Based on customer negotiations, some features are beyond the scope of our project and may be addressed in the future. One such feature is tracking multiple pedestrians. The current product need only worry about tracking one pedestrian at a time. Also, erratic pedestrian movement will not be a factor in our product. The pedestrian will always move at a steady speed. Additionally, since the vehicle is expected to be fully automated, the system has no need to interact with the driver.

1. Specific Requirements
2. The system consists of a pedestrian sensor and a brake-by-wire actuator.
3. The pedestrian sensor will be a stereo camera and will send a packet every 100 ms. The data in the packet contains the pedestrian location (+/- 0.5 m) relative to the car, and the pedestrian speed (+= 0.2 m/s) and direction (+/- 5 deg).
4. The Brake-by-Wire (BBW), when activated, interrupts the steady state velocity control (cruise control) and applies braking torque at all four wheels of the vehicle. It has a deceleration accuracy of +/- 2%, a response time of 200 to reach requested decel, and a response time of 100 ms to release. A maximum deceleration of 0.7 g (1g = 9.81 m/s^2) is possible.
5. The vehicle and the pedestrian for testing the system have the following properties:
6. The vehicle is an autonomous vehicle that has a normal steady state speed of 50 kph (13.9 m/s) and an acceleration back to steady state speed (after auto brake apply) of 0.25 g. The collision zone is based on the vehicle’s width of 2 m.
7. The pedestrian for this application can be in static or in motion and have speeds of 0 kph OR 6 kph and it can be assumed that the pedestrian can change velocity in infinite acceleration. The size of the pedestrian can be considered a circle with 0.5 m diameter.
8. The system sensor should be able to recalculate the braking distance between the vehicle and pedestrian by responding appropriately.
9. The system must return to steady-state velocity after the auto braking maneuver with an acceleration of 0.25 g.
10. When the vehicle is in a potential collision zone, the system should take action immediately to brake automatically and avoid collisions.
11. Based on the scenarios described in the project overview, the system should be tested assuming that is does not know which scenario is occurring.
12. The system should be effective (Zero Collisions allowed) and efficient (minimize lost time).
13. Modeling Requirements

The following Use-Case diagram shows the different interactions available to users of the APCA system. The stick figure of a person symbolizes a user or other external actor, and the arrow that protrudes from them reach ovals that represent high-level actions that a user can take to affect the system’s behavior.

**USE Case Diagram for Part 3**

****

|  |  |
| --- | --- |
| Use Case: | Detects Pedestrian |
| Actors: | Sensor |
| Type: | Primary and Essential |
| Description: | Sensor scans, recognizes and tracks pedestrians in front of it. |
| Cross-references: | 1a, 3, 6, 7 |

|  |  |
| --- | --- |
| Use Case: | Steady State Speed |
| Actors: | Vehicle |
| Type: | Primary and Essential |
| Description: | The Autonomous Vehicle is set to a steady velocity. |
| Cross-references: | 2a, 6, 7 |


|  |  |
| --- | --- |
| Use Case: | Avoids Pedestrian |
| Actors: | Vehicle |
| Type: | Primary and essential |
| Description: | The Autonomous Vehicle moves in forward direction, the sensor detects the pedestrian and avoids collision. |
| Includes: | Automatic Braking (BBW), Return to Steady Speed |
| Cross-references: | 2a, 4, 5, 6, 7 |
| Related Use-Cases: | Activates Automatic Braking (BBW) and Return to Steady State (if necessary) use cases |

|  |  |
| --- | --- |
| Use Case: | Return to Steady State |
| Actors: | Sensor |
| Type: | Primary and Essential |
| Description: | The Sensor detects a pedestrian, the vehicle brakes and avoids collision. Then, the vehicle resumes back to the original set speed. |
| Cross-references: | 2a, 4, 6, 7 |

|  |  |
| --- | --- |
| Use Case: | Automatic Braking (BBW) |
| Actors: | Vehicle |
| Type: | Primary and Essential |
| Description: | Once the pedestrian has been detected, the BBW sub-system responds to deceleration requests and automatically starts braking accordingly until collision has been avoided. |
| Cross-references: | 1b, 3, 5, 6, 7 |


|  |  |
| --- | --- |
| Use Case: | Scan for obstacles |
| Actors: | Pedestrian |
| Type: | Primary and essential |
| Description: | The pedestrian can be in static or in motion, can change speed with infinite acceleration. When moving, the pedestrian only moves in right angle to the vehicles path. |
| Cross-references: | 2b, 6, 7 |

**Class Diagram and Data Dictionary**


****


|  |  |  |  |
| --- | --- | --- | --- |
| **Class** | **Attributes** | **Operations** | **Relationships** |
| ABP System | failSafeMode – a boolean value that will show if the system is in fail safe mode or not. decelerationRate – a double value that will show how fast the vehicle can decelerate. | CalculateLostTime() – an operation that will be run to calculate how much time is lost if and when the vehicle decelerates to avoid a pedestrian. | The ABP System is a subsystem of the Vehicle. |
| Vehicle | velocity – a double value that determines the velocity of the vehicle. | Brake() – an operation that will be called if the car needs to avoid a pedestrian.  Accelerate() – an operation that will be called to bring the vehicle back to its previous speed to cut down on lost time.  AlertOfFailSafe() – If fail safe mode is activated, this operation will alert the driver that the car should be taken in for repair. | The Vehicle contains both the ABP System and the BBW Actuator and uses them to detect and avoid possible pedestrian collisions. |
| Pedestrian Sensor |  | LookForPedestrian() – an operation by the sensor that will constantly scan for pedestrians that the vehicle may collide with. | The Pedestrian Sensor is a subsystem of the ABP System. It scans for Pedestrians that the car may potentially collide with. |
| Pedestrian | velocity – the velocity of the pedestrian. initial X – the starting point of the pedestrian in regards to the X axis.  initial Y – the starting point of the pedestrian in regards to the Y axis.  startTime – the time at which the pedestrian will start walking across the street (if they do). |  | The Pedestrian triggers the Pedestrian Sensor. |
| BBW Actuator |  | ApplyBrakes() – If the vehicle decides to brake, the BBW Actuator will use this operation to slow the vehicle. | The BBW Actuator is a subsystem of the Vehicle. |

Below is a state diagram for the APCA system. The system constantly scans for pedestrians as soon as the vehicle is turned on. For each new pedestrian found, it begins tracking. When a pedestrian steps in front of the car, it is seen as being in danger of collision. A signal is then sent to the BBW actuator and braking is applied. As soon as the pedestrian is out of danger, acceleration begins to bring the vehicle up to speed. During acceleration, the tracking module makes sure no pedestrians enter a collision course. After initial velocity is achieved again, the system calculates time lost due to evasive maneuvers.



Below are sequence diagrams for different scenarios the system may encounter. The first is with no pedestrian present. The vehicle maintains its current velocity and continues as normal. The second scenario is with a pedestrian present. When the pedestrian is in danger of being in a collision, the vehicle brakes until the danger has passed. Then the vehicle accelerates back up to its initial velocity and continues.





1. Prototype

Our prototype consists of 10 defined scenario buttons, and a chart that gives the details of each scenario. It also contains a form that users can input their own custom variables. At the bottom of the web page is a results box.

* 1. How to Run Prototype

To run our prototype, all you need is a web browser that supports JavaScript.

What system configuration? (Should be accessible through web.) Are there

plugins? Are there any OS or networking constraints. Give the URL for the

prototype.

* 1. Sample Scenarios

Our Prototype currently does not execute, but following is an example of how we plan on it working. The customer arrives to our webpage and is presented with a table containing all the information of the predefined scenarios we are supposed to test for. Beneath the table are 10 buttons, one for each predefined scenario. Upon clicking the button, we will run our algorithm on the variables to determine if the pedestrian is hit or not, and what the loss of time for each scenario will be. This information will be displayed in the “Results” box at the bottom of the page. There is also a form that allows for custom scenarios to be run. The customer will be able to plug in numbers to the text boxes and click the “Compute Scenario” button to test the system under any conditions.

1. References

Provide list of all documents referenced in the SRS

Identify each document by title, report number, date, and publishing organization.

Specify the sources from which the references can be obtained.

Include an entry for your project website.

Start of your text.

1. D. Thakore and S. Biswas, “Routing with Persistent Link Modeling in Intermittently Connected Wireless Networks,” Proceedings of IEEE Military Communication, Atlantic City, October 2005.
2. Point of Contact

For further information regarding this document and project, please contact **Prof. Betty H.C. Cheng** at Michigan State University (chengb at cse.msu.edu). All materials in this document have been sanitized for proprietary data. The students and the instructor gratefully acknowledge the participation of our industrial collaborators.